**Data From BPS for Import from China ( In Tons )**

|  |  |  |  |
| --- | --- | --- | --- |
| Commodity | 2015 | 2016 | 2017 |
| Ceramic Tile | 837,137 | 1,061,514 | 1,211,914 |

**Import Ceramic Tile From India ( in USD )**

|  |  |  |
| --- | --- | --- |
| **HSCode** | **Commodity** | **2015-2016**  |
| 69010030 | TILES    | 0.08 |
|   | Total  | 0.08 |

|  |  |  |
| --- | --- | --- |
| **HSCode** | **Commodity** | **2016-2017**  |
| 69010030 | TILES    | 0.03 |
| 69071090 | \*TILES OTHR THAN VITRIFIED TILES    | 0 |
| 69081020 | \*CERAMIC MOSAIC TILES    | 0 |
|   | Total | 0.03 |

|  |  |  |
| --- | --- | --- |
| **HSCode** | **Commodity** | **2017-2018**  |
| 69010030 | TILES    | 0.01 |
| 69071090 | \*TILES OTHR THAN VITRIFIED TILES    |    |
| 69081020 | \*CERAMIC MOSAIC TILES    |    |
|   | Total | 0.01 |

BPS Data of Ceramic Tile Import from All Country ( In USD )

|  |  |  |
| --- | --- | --- |
| **Kode HS** | **Deskripsi HS** | **Jan 2015 - Dec 2016** |
| 6901000000 | Bricks.blocks.tiles & oth ceramic goods | 166,718 |
| 6905100000 | Roofing tiles of ceramic | 581,673 |
| 6907901000 | Paving.hearth/wall tiles.rectangle. | 158,983,006 |
| 6907902000 | Lining tiles of a kind used for grinding | 75,538 |
| 6907909000 | Oth thn tile.cube&similar article. | 117,487 |
| 6908101000 | Paving.hearth/wall tiles.rectangle. | 3,128,147 |
| 6908109000 | Oth thn Paving.hearth/wall tiles. | 93,098 |
| 6908901100 | Paving.hearth/wall tiles of plain tiles. | 581,374 |
| 6908901900 | Oth thn paving.hearth/wall tiles of plai | 8,561 |
| 6908909100 | Paving.hearth/wall tile of oth | 28,163,038 |
| 6908909900 | Oth thn paving.hearth/wall tile of oth | 218,465 |
|   | Total | 192,117,105 |
| **Kode HS** | **Deskripsi HS** | **Jan 2016 - Dec 2016** |
| 6901000000 | Bricks,blocks,tiles & oth ceramic goods | 39,794 |
| 6905100000 | Roofing tiles of ceramic | 489,627 |
| 6907101000 | Paving,hearth/wall tiles,rectangle, | 198,974 |
| 6907109000 | Oth thn Paving,hearth/wall tiles, | 9,710 |
| 6907901000 | Paving,hearth/wall tiles,rectangle, | 180,934,008 |
| 6907902000 | Lining tiles of a kind used for grinding | 32,274 |
| 6907909000 | Oth thn tile,cube&similar article, | 24,488 |
| 6908101000 | Paving,hearth/wall tiles,rectangle, | 1,894,581 |
| 6908109000 | Oth thn Paving,hearth/wall tiles, | 73,926 |
| 6908901100 | Paving,hearth/wall tiles of plain tiles, | 1,152,740 |
| 6908901900 | Oth thn paving,hearth/wall tiles of plai | 36,438 |
| 6908909100 | Paving,hearth/wall tile of oth | 29,909,426 |
| 6908909900 | Oth thn paving,hearth/wall tile of oth | 129,231 |
|   | Total | 214,925,217 |

|  |  |  |
| --- | --- | --- |
| **Kode HS** | **Deskripsi HS** | **Jan 2017 - Dec 2018** |
| 69010000 | Bricks,blocks,tiles&oth ceramic goods of siliceous fossilmeals/of similar siliceous earths | 99,222 |
| 69049000 | Flooring blocks,support/filler tiles&the like | 204,335 |
| 69051000 | Roofing tiles of ceramic | 677,950 |
| 69072110 | Lining tiles of a kind use for grinding mills,unglazed,water absorption coeff by weight<= 0.5 % | 307,033 |
| 69072123 | Pving,wall tiles,glaze,largest surface area capablesquare side<= 0.5 % | 140,076 |
| 69072124 | Ceramic,wall tiles,glaze ,large surfce area capablesquare side<= 0.5 % | 6,282 |
| 69072191 | Paving,wall tiles,unglaze ,large surface area capablesquare side>7 cm water absorption coeff by weight<= 0.5 % | 201,149,419 |
| 69072193 | Paving,wall tiles,glaze ,large surface area capablesquare side>7cm water absorption coeff by weight<= 0.5 % | 39,920,222 |
| 69072194 | Ceramic,wall tiles,glaze ,large surface area capablesquare side>7cm water absorption coeff by weight<= 0.5 % | 75,165 |
| 69072211 | Pving,wall tiles,unglazed ,large surfce area capable square side<=10% | 9,806 |
| 69072291 | Paving,wall tiles,unglaze ,large surface which capable square side>7cm of water absorp 0.5%<=10% | 147,867 |
| 69072293 | Pving,wall tiles,glaze , largst surfce area capable square side>7cm of waterabsorp 0.5%<=10% | 1,756,283 |
| 69072313 | Paving,wall tiles,glaze ,large surface area capable square side10% | 1,264,113 |
| 69072314 | Ceramic,wall tiles,glaze ,large surface area capble square side10% | 16,953 |
| 69072391 | Paving,wall tiles,unglaze ,large surface area capable square side>7 cm of water absorp coeff weight>10% | 210,054 |
| 69072393 | Paving,wall tiles,glaze ,large surface area capable square side>7 cm of water absorp coeff weight>10% | 2,961,989 |
|   | Total | 248,946,769 |

|  |  |  |
| --- | --- | --- |
| **Kode HS** | **Deskripsi HS** | **Jan 2018 - Jul 2018** |
| 69010000 | Bricks,blocks,tiles&oth ceramic goods of siliceous fossilmeals/of similar siliceous earths | 46,776 |
| 69049000 | Flooring blocks,support/filler tiles&the like | 28,633 |
| 69051000 | Roofing tiles of ceramic | 319,845 |
| 69072110 | Lining tiles of a kind use for grinding mills,unglazed,water absorption coeff by weight<= 0.5 % | 94,407 |
| 69072121 | Flag&paving,hearth/wall tile,oth than of subhead 6907.30&6907.40 water absorption coeff by weight<=0.5 % | 899 |
| 69072122 | Ceramic,wall tile,unglaze,large surface area capablesquare side<= 0.5 % | 859 |
| 69072123 | Pving,wall tiles,glaze,largest surface area capablesquare side<= 0.5 % | 1,982 |
| 69072124 | Ceramic,wall tiles,glaze ,large surfce area capablesquare side<= 0.5 % | 38,520 |
| 69072191 | Paving,wall tiles,unglaze ,large surface area capablesquare side>7 cm water absorption coeff by weight<= 0.5 % | 136,112,625 |
| 69072192 | Ceramic,wall tile,unglaze ,large surface area capablesquare side>7cm water absorption coeff by weight<= 0.5 % | 10,344 |
| 69072193 | Paving,wall tiles,glaze ,large surface area capablesquare side>7cm water absorption coeff by weight<= 0.5 % | 36,035,438 |
| 69072194 | Ceramic,wall tiles,glaze ,large surface area capablesquare side>7cm water absorption coeff by weight<= 0.5 % | 13,684 |
| 69072291 | Paving,wall tiles,unglaze ,large surface which capable square side>7cm of water absorp 0.5%<=10% | 4,361 |
| 69072292 | Ceramic,wall tiles,unglaze,large surfce area capable square side>7cm of water absorp 0.5%<=10% | 117 |
| 69072293 | Pving,wall tiles,glaze , largst surfce area capable square side>7cm of waterabsorp 0.5%<=10% | 1,714,916 |
| 69072294 | Ceramic,wall tiles,glaze ,large surface area capable square side>7cm of water absorp 0.5%<=10% | 221 |
| 69072313 | Paving,wall tiles,glaze ,large surface area capable square side10% | 603,705 |
| 69072314 | Ceramic,wall tiles,glaze ,large surface area capble square side10% | 1,542 |
| 69072392 | Ceramic,wall tile,unglaze ,large surface area capable square side>7cm of water absorp coeff weight>10% | 39 |
| 69072393 | Paving,wall tiles,glaze ,large surface area capable square side>7 cm of water absorp coeff weight>10% | 1,568,832 |
| 69072394 | Ceramic,wall tiles,glaze ,large surface area capble square side>7cm of water absorp coeff weight>10% | 4,177 |
|   | Total | 176,601,922 |